Technical Data Sheet

Formerly Known As: Shell Alvania Grease EP(LF) 2, Shell Retinax EP 2

Shell Gadus ***S2*** ***V220*** ***2***

***High*** ***Performance*** ***Multipurpose*** ***Extreme*** ***Pressure*** ***Grease***

* *Reliable* *Protection*
* *Multi-purpose* *Applications*
* *Lithium*

Shell Gadus S2 V220 greases are high quality multipurpose, extreme-pressure greases based on a blend of high viscosity index mineral oils and a lithium hydroxystearate soap thickener and contain extreme-pressure and other proven additives to enhance their performance in a wide range of applications.

Shell Gadus S2 V220 greases are designed for multipurpose grease lubrication of rolling element and plain bearings as well as hinges and sliding surfaces such as those found in throughout most industrial and transport sectors.



# Performance, Features & Benefits

* Outstanding Load Carrying Capacity

Shell Gadus S2 V220 greases contain special extreme- pressure additives which enable them to withstand heavy and shock loads without failure of the lubricant film.

* Improved Mechanical Stability

This is particularly important in vibrating environments where poor mechanical stability can lead to grease softening with subsequent loss of lubrication performance and leakage.

* Good Resistance to Water Wash-out

Shell Gadus S2 V220 greases have been formulated to offer resistance to water wash-out.

* Oxidation Stability

Specially selected base oil components have excellent oxidation resistance. Their consistency will not alter in storage and they withstand high operating temperatures without hardening or forming bearing deposits.

* Good Corrosion Resistance Characteristics

Shell Gadus S2 V220 greases reliably protect bearing surfaces against corrosion, even when a high amount of water is present.

# Typical physical characteristics

Main Applications





Shell Gadus S2 V220 2 greases are designed for:

* Heavy duty bearings and general industrial lubrication.
* Heavy duty plain and rolling element bearings operating

under harsh conditions including shock loading in wet

environments.

# Specifications, Approvals & Recommendations

For a full listing of equipment approvals and recommendations, please consult your local Shell Technical Helpdesk.

|  |  |  |
| --- | --- | --- |
| Properties | Method | Shell Gadus S2 V220 2 |
| NLGI Consistency |  | 2 |
| Soap Type |  | Lithium |
| Base Oil |  | Mineral |
| Kinematic Viscosity @400C cSt | IP 71 / ASTM D445 | 220 |

|  |  |  |
| --- | --- | --- |
| Properties | Method | Shell Gadus S2 V220 2 |
| Kinematic Viscosity @1000C cSt | IP 71 / ASTM D445 | 19 |
| Cone Penetration, Worked @250C 0.1mm | IP 50 / ASTM D217 | 265-295 |
| Dropping Point 0C | IP 396 | 180 |
| Four Ball Weld Load kg | ASTM D2596 | 315 |

These characteristics are typical of current production. While future production will conform to Shell's specification, variations in these characteristics may occur.

# Health, Safety & Environment

·Health and Safety

Shell Gadus S2 V220 Grease is unlikely to present any significant health or safety hazard when properly used in the recommended application and good standards of personal hygiene are maintained.

Avoid contact with skin. Use impervious gloves with used oil. After skin contact, wash immediately with soap and water.

Guidance on Health and Safety is available on the appropriate Safety Data Sheet, which can be obtained from <http://www.epc.shell.com/>

* Hydraulic Brake Rubber Components

Care should be taken to ensure that the grease does NOT come into contact with hydraulic brake rubber components.

* Protect the Environment

Take used oil to an authorized collection point. Do not discharge into drains, soil or water.

# Additional Information

* Operating Temperature

Shell Gadus S2 V220 2 is recommended for the operating temperature range -200C to +1300C.

* Re-greasing Intervals

For bearings operating near their maximum recommended temperatures, re-greasing intervals should be reviewed.

* Advice

Advice on applications not covered here may be obtained from your Shell representative.

[Visit SCL](http://shop.sclubricants.com/gadus-s2-v220-2) <http://shop.sclubricants.com/gadus-s2-v220-2>